Experiments to be done

1. Notched Three Point Bending test. (ASTM D790 ASTM E1290)
2. Hopkinson Bar Experiment.
3. Flexural Strength test.
4. Compressive Strength test.
5. SEM and XRD.